display_name = "Sega - Dreamcast/NAOMI (Reicast)"
authors = "skmp|flyinghead"
supported_extensions = "chd|cdi|iso|elf|bin|cue|gdi|lst|zip|dat|7z"
corename = "Reicast"
manufacturer = "Sega"
categories = "Emulator"
systemname = "Sega Dreamcast"
systemid = "dreamcast"
database = "Sega - Dreamcast|Sega - NAOMI"
license = "GPLv2"
permissions = ""
display_version = "Git"
supports_no_game = "false"
firmware_count = 8
firmware0_desc = "dc_boot.bin (Dreamcast BIOS)"
firmware0_path = "dc/dc_boot.bin"
firmware0_opt = "false"
firmware1_desc = "dc_flash.bin (Date/Time/Language)"
firmware1_path = "dc/dc_flash.bin"
firmware1_opt = "false"
firmware2_desc = "naomi.zip (Naomi Bios from MAME)"
firmware2_path = "dc/naomi.zip"
firmware2_opt  = "true"
firmware3_desc = "hod2bios.zip (Naomi The House of the Dead 2 Bios from MAME)"
firmware3_path = "dc/hod2bios.zip"
firmware3_opt  = "true"
firmware4_desc = "f355dlx.zip (Naomi Ferrari F355 Challenge deluxe Bios from MAME)"
firmware4_path = "dc/f355dlx.zip"
firmware4_opt  = "true"
firmware5_desc = "f355bios.zip (Naomi Ferrari F355 Challenge twin/deluxe Bios from MAME)"
firmware5_path = "dc/f355bios.zip"
firmware5_opt  = "true"
firmware6_desc = "airlbios.zip (Naomi Airline Pilots deluxe Bios from MAME)"
firmware6_path = "dc/airlbios.zip"
firmware6_opt  = "true"
firmware7_desc = "awbios.zip (Atomiswave BIOS from MAME)"
firmware7_path = "dc/awbios.zip"
firmware7_opt  = "true"
notes = "(!) dc_boot.bin (md5): e10c53c2f8b90bab96ead2d368858623|(!) dc_flash.bin (md5): 0a93f7940c455905bea6e392dfde92a4|(!) naomi.zip (md5): eb4099aeb42ef089cfe94f8fe95e51f6|(!) hod2bios.zip (md5): 9c755171b222fb1f4e1439d5b709dbf1|(!) f355dlx.zip (md5): 5e83867c751f692a000afdf658dc181f|(!) f355bios.zip (md5): f126d318f135f38ee377fef2acf08d7e|(!) airlbios.zip (md5): 3f348c88af99a40fbd11fa435f28c69d|(!) awbios.zip (md5): 0ec5ae5b5a5c4959fa8b43fcf8687f7c"
